- Main
- Tutorials
- Library
- Samples

- File List
- Globals

Namespaces | Functions | Variables
misc.py File Reference

Miscellaneous Sample More...

Go to the source code of this file.

## Namespaces
| misc

## Functions
def | main ()

## Variables
int | LED_CHANNEL_U1 = 1
int | LED_CHANNEL_U2 = 2
int | LED_STATE_DARK = 0
int | LED_STATE_GREEN = 1
int | LED_STATE_RED = 2

## Detailed Description

Miscellaneous Sample

Copyright
  2019 Moxa Inc. All rights reserved.

Date
  2019-02-11

Author
  William Chang

Version
  V1.0

Library:
Misc APIs

1 '''
2 Copyright (C) 2019 Moxa Inc. All rights reserved.
3 SPDX-License-Identifier: Apache-2.0
4
5 Miscellaneous Python Sample Application
6
7 Date Author Comment
8 2019-02-11 William Chang Created it.
9 '''
10
11
21
22 from ioThinx_4530 import ioThinx_4530_API
23 import argparse
24
25 LED_CHANNEL_U1 = 1
26 LED_CHANNEL_U2 = 2
27 LED_STATE_DARK = 0
28 LED_STATE_GREEN = 1
29 LED_STATE_RED = 2
30
31
32 def main():
33 parser = argparse.ArgumentParser(description="Miscellaneous sample program.")
34 parser.add_argument("-s", "--slot", dest="module_slot", type=int, default=1)
35 args = parser.parse_args()
36
37 # initialize ioThinx I/O
38 misc_slot = 0
39 module_slot = args.module_slot
40 device = ioThinx_4530_API.ioThinx_4530_API()
41
42 # module infomation
43 module_count = device.ioThinx_Misc_GetModuleCount()
44 print("Module count = {}".format(module_count))
45 print("Module slot = {}".format(module_slot))
46
47 module_info = device.ioThinx_Misc_GetModuleInfo(module_slot)
48 print("Slot {} Module Information:".format(module_slot))
49 print("Model Name: {}".format(module_info["model_name"]))
50 print("Serial Number: {}".format(module_info["serial_number"]))
51
52 # locating
53 device.ioThinx_Misc_SetLocateState(module_slot, 1)
54 print("Slot {}: Locating...".format(module_slot))
55 input("Press enter to stop locate.")
56 device.ioThinx_Misc_SetLocateState(module_slot, 0)
57 rs_state = device.ioThinx_Misc_GetRotarySwitchState(misc_slot)
58 print("Rotary switch state = {}".format(rs_state))
59
60 # push button
61 pbtn_state = device.ioThinx_Misc_GetPushButtonState(misc_slot)
62 print("Push button state = {}".format(pbtn_state))
63
64 # user led
65 device.ioThinx_Misc_SetUserLedState(misc_slot, LED_CHANNEL_U1, LED_STATE_GREEN)
66 print("Set LED U1 to GREEN")
67 device.ioThinx_Misc_SetUserLedState(misc_slot, LED_CHANNEL_U2, LED_STATE_RED)
68 print("Set LED U2 to RED")
69 input("Press enter to clear.")
70 device.ioThinx_Misc_SetUserLedState(misc_slot, LED_CHANNEL_U1, LED_STATE_DARK)
71 device.ioThinx_Misc_SetUserLedState(misc_slot, LED_CHANNEL_U2, LED_STATE_DARK)
72 input("Press enter to continue.")
73
74
75 if __name__ == '__main__':
76 main()

Definition in file misc.py.