- Main
- Tutorials
- Library
- Samples

ioThinx Controllers Documentation

This programming guide describes the C/C++, python, cloud connectivity libraries and sample codes provided with ioThinx controllers. The purpose of this guide is to help users to learn how to program the ioThinx controllers more easily. Additional information about ioThinx features is available in the following manuals, which can be found on the ioThinx Documentation & Software CD.

    - ioThinx 4533-LX Hardware User's Manual
    - ioThinx 4533-LX Software User's Manual

This guide supports the following products:

    - ioThinx 4533-LX
    - 45ML-5401, 45ML-5401-T (Serial, 4 Channels)
    - 45MR-1600, 45MR-1600-T (DI, 16 Channels, PNP + Dry, 24 VDC)
    - 45MR-1601, 45MR-1601-T (DI, 16 Channels, NPN + Dry, 24 VDC)
    - 45MR-2600, 45MR-2600-T (DO, 16 Channels, Sink, 24 VDC)
    - 45MR-2601, 45MR-2601-T (DO, 16 Channels, Source, 24 VDC)
    - 45MR-2606, 45MR-2606-T (DI, 8 Channels, PNP + Dry, 24 VDC, DO, 8 Channels, Source, 24 VDC)
    - 45MR-2404, 45MR-2404-T (Relay, 4 Channels, Form A (N.O.), 2A @ 30 VDC, 250 VAC)
    - 45MR-3800, 45MR-3800-T (AI, 8 Channels, 16 bits, 0 to 20 mA, 4 to 20 mA)
    - 45MR-3810, 45MR-3810-T (AI, 8 Channels, 16 bits, 0 to 10 VDC, -10 to 10 VDC)
    - 45MR-4420, 45MR-4420-T (AO, 4 Channels, 12 bits, 0 to 10 VDC, 0 to 20 mA, 4 to 20 mA)
    - 45MR-6600, 45MR-6600-T (RTD, 6 Channels)
    - 45MR-6810, 45MR-6810-T (TC, 8 Channels)
    - 45MR-7210, 45MR-7210-T (Power, 5W, 12 to 48VDC)

Release Note