- Main
- Tutorials
- Library
- Samples

- Namespace List
- Namespace Members

Functions
relay Namespace Reference

## Functions
def | main ()

## Detailed Description

    Copyright (C) 2019 Moxa Inc. All rights reserved.
    SPDX-License-Identifier: Apache-2.0

    Relay Python Sample Application

    Date          Author            Comment
    2019-02-11    William Chang     Created it.

## Function Documentation

def relay.main | ( |  | ) |

Definition at line 26 of file relay.py.

26 def main():
27 parser = argparse.ArgumentParser(description="Relay sample program.")
28 parser.add_argument("-s", "--slot", dest="relay_slot", type=int, default=6)
29 parser.add_argument("-c", "--channel", dest="relay_channel", type=int, default=3)
30 args = parser.parse_args()
31
32 relay_slot = args.relay_slot
33 relay_channel = args.relay_channel
34 relay_values = 0
35 print("Relay slot = {}", relay_slot)
36 print("Relay channel = {}", relay_channel)
37
38 # initialize ioThinx I/O
39 device = ioThinx_4530_API.ioThinx_4530_API()
40 relay_values = device.ioThinx_Relay_GetValues(relay_slot)
41 print(relay_values)
42
43 # set value
44 while True:
45 # invert relay value
46 relay_values[relay_channel] = 0 if relay_values[relay_channel] == 1 else 1
47
48 device.ioThinx_Relay_SetValues(relay_slot, relay_values)
49 print("[ {}:{}] relay value = {}".format(relay_slot, relay_channel, relay_values))
50
51 relay_count = device.ioThinx_Relay_GetCurrentCounts(relay_slot, relay_channel, 1)
52 print("[ {}:{}] relay count = {}".format(relay_slot, relay_channel, relay_count))
53 if input("Press 'q' to exit. other keys to continue") == 'q':
54 break
55
56
relay.main
def main()
Definition: relay.py:26
format
char const int const cJSON_bool format
Definition: cJSON.h:161